1. Home
2. Products
3. Cardio Machine
4. Indoor Cycling Bike
5. MS5811 Indoor Cycling Bike

## MS5811 Indoor Cycling Bike

- Indoor cycling bike with screen: MS5811-TFT
- Indoor cycling bike without screen: MS5811

MS Fitness provides two kinds of MS5811 indoor cycling bike
The MS5811 indoor cycling bike which is not equipped with a standard screen and the MS5811-TFT indoor cycling bike which is equipped with a touch screen.

Suitable crowd
The MS-5811 indoor cycling bike is specially designed according to the biomechanical characteristics of the human body. The bike is a great choice for users of all body sizes and shapes.

Parameter
1. Scope of application

Maximum user weight | 150KG
Up and down adjusting stroke of the handlebar | 160MM
Maximum adjusting height of the handlebar | 1100MM
Up and down adjusting stroke of the seat | 190MM
Front and rear adjusting stroke of the saddle | 110MM
Maximum adjusting stroke of the saddle | 1170MM

2. Size and weight

Length | 1665MM
Width | 705MM
Height | 1445MM
Weight | 86KG
Gross Weight | 96KG

Configuration information
● The frame ergonomically designed. The tightness of the foot cover is adjustable. The cushion is adjustable up and down, from front to rear. The handrail is also adjustable up and down.
● The indoor cycling bike is clipper-built. And it adopts a 50*80 rectangular tube and 50*120 flat ellipse tube as its body. High quality aluminum alloy slideway as its adjusting tube and adjusting slideway.
● This kind of cardio equipment adopts the thickened medial axis and high-strength pedal in order to decrease failure rate and extend the service life.
● The user can choose the belt drive or the chain drive. And the product is bidirectional rotating.
● This fitness equipment weighs 86kg. And it's equipped with a 20kg flywheel for stability.
● This kind of cardio equipment features a magnetron round brake which is made of a smooth texture as its inertia wheel, and adopts the design of down pressure brake to decrease the loss of the brake system.
● This equipment adopts the unique designed protective cover to protect the flywheel from corrosion from sweat.
● Handlebars can be adjusted smoothly and it is also high-stability and resistant to corrosion.
● Our indoor cycling bike is equipped with a bottle cage on the frame.
● The resistance mode is magnetic resistance, the user can choose the stepless resistance and the brake systems as the resistance adjusting mode.

All MS Fitness equipment is delivered with an operating and installation manual. Our staff members can install equipment upon request and if conditions permit.

Related products

- MS5811 Indoor Cycling Bike
- MS5809 Indoor Cycling Bike

Inquiry Form
Other Products

- 2. MS5809 Indoor Cycling Bike
- 2. Magnetic Upright Exercise Bike
- 2. Magnetic Recumbent Exercise Bike
- 2. Elliptical Trainer Machine